Zublin_ETS-DB_readme.txt
2.12.2016/cfs 

KNX-FW revision vs ETS-ProductData for Niko-Zublin KNX Presence-Detectors
*************************************************************************
SG: SwissGarde, P: Presence, KLR: ConstantLightControl, FW: Firmware

ArtNr     	 Produkt             			  ¦#PIR ¦ FW-Rev      ¦ Prod.Code*          ¦ ETS-DB Datei
--------------------------------------------------------------------------------------------------------

350-41730to35	 Servodan 3-Zonen Tageslichtregelung	  ¦  3  ¦ all	      ¦ 		    ¦ 350-41730 - 350-41735 Servodan.knxprod

350-34001to04	 P34/M34 KNX/KLR			  ¦ 1-3 ¦ v0.1 to 1.97¦ 		    ¦ 350-34001 - 350-34004 Niko P34-M34 bis FW 1.97.knxprod
350-34001to04	 P34/M34 KNX/KLR			  ¦ 1-3 ¦ v2.5 and >  ¦ 		    ¦ 350-34001 - 350-34004 Niko P34-M34 ab  FW 2.50.knxprod

350-213001	 Outdoor KNX 				  ¦  3  ¦ all	      ¦ 		    ¦ 350-213001 Outdoor detector.knxprod

350-530311	 Corridor KNX				  ¦  3  ¦ all	      ¦ 		    ¦ 350-530311 Corridor KNX detector.knxprod

360-31001	 RF Dimmer KNX				  ¦  -  ¦ all	      ¦ 		    ¦ 360-31001 KNX RF Dimmer switch_v1.1.knxprod

360-33001	 RF Media Coupler KNX			  ¦  -  ¦ all	      ¦ 		    ¦ 360-33001 KNX RF Media Coupler_v1.0.knxprod

11500		 12CH Multi IO KNX			  ¦  -  ¦ all	      ¦ 		    ¦ 11500 12-CH_Multi-IO.vd4

11501		 USB Interface KNX			  ¦  -  ¦ all	      ¦ 		    ¦ 11501 USB_Interface.vd4

11502		 Media Coupler KNX			  ¦  -  ¦ all	      ¦ 		    ¦ 11502 Media_Coupler.vd4

11503		 Binary Input KNX			  ¦  -  ¦ all	      ¦ 		    ¦ 11503 Binary_Input_4xIN.vd4

25010      	 SG Hokuspokus KNX/KLR			  ¦  2  ¦ v2.4 to 2.6 ¦ xxxDxxx to xxxFxxx  ¦ 25010 Hokuspokus V2.4.vd4    
25010     	 SG Hokuspokus KNX/KLR 			  ¦  2  ¦ v2.7 and >  ¦ xxxGxxx and greater ¦ 25010 Hokuspokus V2.7.vd4  

25020N    	 SG360P KNX UP        			  ¦  4  ¦ v2.2 and >  ¦ xxxBxxx to xxxCxxx  ¦ 25020N SG360_4PIR_V2.2.vd4
25030     	 SG360P KNX/KLR UP   			  ¦  4  ¦ v2.2 and >  ¦ xxxBxxx and greater ¦ 25030 SG360P_4PIR_V2.2.vd4

25032to37 	 SG360P KNX/KLR      			  ¦  3  ¦ v2.4 to 2.6 ¦ xxxDxxx to xxxFxxx  ¦ 25032 - 25037 SG360_3PIR_V2.4.vd4  
25032to37  	 SG360P KNX/KLR     		          ¦  3  ¦ v2.7 and >  ¦ xxxGxxx and greater ¦ 25032 - 25037 SG360_3PIR_V2.7.vd4

25038to39 	 SG360P KNX/KLR 4-CH  			  ¦  4  ¦ v2.4 to 2.6 ¦ xxxDxxx to xxxFxxx  ¦ 25038 - 25039 SG360_4PIR_V2.4.vd4  
25038to39  	 SG360P KNX/KLR 4-CH   			  ¦  4  ¦ v2.7 and >  ¦ xxxGxxx and greater ¦ 25038 - 25039 SG360_4PIR_V2.7.vd4

25240to49 	 SG300P KNX/KLR        			  ¦  3  ¦ v2.4 to 2.6 ¦ xxxDxxx to xxxFxxx  ¦ 25240 - 25249 SG300_3PIR_V2.4.vd4
25240to49 	 SG300P KNX/KLR      			  ¦  3  ¦ v2.7 and >  ¦ xxxGxxx and greater ¦ 25240 - 25249 SG300_3PIR_V2.7.vd4

Remark: 
- ETS-DB v2.4 and v2.7 are downwards compatible 
- for full functionality use/replace the ETS-DB that match FW-Rev, as listed above
- after installation/replacement is recommendet to calibrate the brightness value with ETS (see Application Description)  

*ProductionCode is beside the TypePlate on a small silver-white label. 
Examples (Prod.Code allways with 7 characters): 
46EF032 => xxxFxxx, F means FW-v2.6
03FH010 => xxxHxxx, H means FW-v2.8
C = v2.3; D = v2.4; E = v2.5; F = v2.6; 
G = v2.7; H = v2.8; I = v2.9; J = v3.0;

#end of file   		   